=====================================
Server Discovery And Monitoring Tests
=====================================

The YAML and JSON files in this directory tree are platform-independent tests
that drivers can use to prove their conformance to the
Server Discovery And Monitoring Spec.

Version
-------

Files in the "specifications" repository have no version scheme. They are not
tied to a MongoDB server version.

Format
------

Each YAML file has the following keys:

- description: Some text.
- uri: A connection string.
- phases: An array of "phase" objects.

A "phase" of the test sends inputs to the client, then tests the client's
resulting TopologyDescription. Each phase object has two keys:

- responses: An array of "response" objects.
- outcome: An "outcome" object representing the TopologyDescription.

A response is a pair of values:

- The source, for example "a:27017".
  This is the address the client sent the "ismaster" command to.
- An ismaster response, for example `{ok: 1, ismaster: true}`.
  If the response includes an electionId it is shown in extended JSON like
  `{"$oid": "000000000000000000000002"}`.
  The empty response `{}` indicates a network error
  when attempting to call "ismaster".

An "outcome" represents the correct TopologyDescription that results from
processing the responses in the phases so far. It has the following keys:

- topologyType: A string like "ReplicaSetNoPrimary".
- setName: A string with the expected replica set name, or null.
- servers: An object whose keys are addresses like "a:27017", and whose values
  are "server" objects.
- logicalSessionTimeoutMinutes: null or an integer.
- maxSetVersion: absent or an integer.
- maxElectionId: absent or a BSON ObjectId.
- compatible: absent or a bool.

A "server" object represents a correct ServerDescription within the client's
current TopologyDescription. It has the following keys:

- type: A ServerType name, like "RSSecondary".
- setName: A string with the expected replica set name, or null.
- setVersion: absent or an integer.
- electionId: absent, null, or an ObjectId.
- logicalSessionTimeoutMinutes: absent, null, or an integer.
- minWireVersion: absent or an integer.
- maxWireVersion: absent or an integer.

Use as unittests
----------------

Mocking
~~~~~~~

Drivers should be able to test their server discovery and monitoring logic
without any network I/O, by parsing ismaster responses from the test file
and passing them into the driver code. Parts of the client and monitoring
code may need to be mocked or subclassed to achieve this. `A reference
implementation for PyMongo 3.x is available here
<https://github.com/mongodb/mongo-python-driver/blob/3.0-dev/test/test_discovery_and_monitoring.py>`_.

Initialization
~~~~~~~~~~~~~~

For each file, create a fresh client object initialized with the file's "uri".

All files in the "single" directory include a connection string with one host
and no "replicaSet" option.
Set the client's initial TopologyType to Single, however that is achieved using the client's API.
(The spec says "The user MUST be able to set the initial TopologyType to Single"
without specifying how.)

All files in the "sharded" directory include a connection string with multiple hosts
and no "replicaSet" option.
Set the client's initial TopologyType to Unknown or Sharded, depending on the client's API.

All files in the "rs" directory include a connection string with a "replicaSet" option.
Set the client's initial TopologyType to ReplicaSetNoPrimary.
(For most clients, parsing a connection string with a "replicaSet" option
automatically sets the TopologyType to ReplicaSetNoPrimary.)

Test Phases
~~~~~~~~~~~

For each phase in the file, parse the "responses" array.
Pass in the responses in order to the driver code.
If a response is the empty object `{}`, simulate a network error.

Once all responses are processed, assert that the phase's "outcome" object
is equivalent to the driver's current TopologyDescription.

Some fields such as "logicalSessionTimeoutMinutes" or "compatible" were added
later and haven't been added to all test files. If these fields are present,
test that they are equivalent to the fields of the driver's current
TopologyDescription.

Continue until all phases have been executed.
