The Win32 version of the "Blinky" example is now located in the directory:

examples\arm-cm\blinky_ek-tm4c123gxl\win32\

This co-location of the Win32 emulation with the embedded code running
on the actual board demonstrates better the "dual targeting" development
approach.