About this Example

==================

This directory contains the "DPP" (Dining Philosopher Problem) QP example
application for the EK-TM4C123GXL board (TivaC LauchPad). This directory
contains portable code that should compile with any C compiler for ARM
Cortex-M.

The sub-directories contain code and project files, which are
specific to the particular ARM toolchains, such as ARM (MDK-ARM),
GCC, and IAR.

Please refer to the README files in the sub-directories for specific
instructions how to use and customize the example to your needs.


Support Code for EK-TM4C123GXL Board 
====================================
The directory qpc\3rd_party\ek-tm4c123gxl contains the CMSIS-
compliant device code for the TM4C123GH6PM MCU. Please see the README
file in this folder for more details.


QS Software Tracing Instrumentation
===================================
This example provides the "Spy" build configuration, which outputs
the QS (Quantum Spy) software tracing data through UART0, which is
connected to the virtual COM port of the TI Stellaris debugger.

The output is generated at 115200 baud rate.

Here is an example invocation of the QSPY host application to receive
the QS data from EK-TM4C123GXL:

qspy -cCOM1

The actual COM port number might be different on your Windows machine.
Please check the Device Manager to find the COM port number.
