About this Example

==================

This directory contains the "Fly 'n' Shoot" game example application for
the EK-LM3S811 board. This directory contains portable code that should
compile with any C/C++ compiler for ARM Cortex-M.

The sub-directories contain code and project files, which are specific to
the particular ARM toolchains, such as ARM (MDK-ARM), GNU, and IAR.

Please refer to the README files in the sub-directories for specific
instructions how to use and customize the example to your needs.


Support Code for EK-LM3S811 Board 
----------------------------------
The directory 3rd_party\ek-lm3s811 contains the CMSIS-compliant
device code for the LM3S811 MCU. Please see the README file in this
folder for more details.


QS Software Tracing Instrumentation
-----------------------------------
The Blinky example provides the "Spy" build configuration, which
outputs the QS (Quantum Spy) software tracing data through UART0,
which is connected to the virtual COM port of the TI Stellaris debugger.

The output is generated at 115200 baud rate.

Here is an example invocation of the QSPY host application to receive
the QS data from EK-TM4C123GXL:

qspy -cCOM1

The actual COM port number might be different on your Windows machine.
Please check the Device Manager to find the COM port number.

